
**Secondary Roads Department APPLICATION FOR**

****

**19501 HWY 64, P.O. Box 368 ANNUAL OVERSIZE PERMIT**

**Anamosa, IA 52205**

**Telephone: (319) 462-3785** **Application No.: T-**

**Email:** [**engineer@co.jones.ia.us**](mailto:engineer@co.jones.ia.us) **Application Fee: $50.00**

APPLICANT INFORMATION (PLEASE PRINT CLEARLY OR TYPE)

Vehicle Owner or Lessee: Requested Start Date:

Mailing Address:

(Street Address) (City) (State) (Zip)

Phone Number: Email Address:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| POWER UNIT INFORMATION | | | | | |
| Plate | State | Vehicle Identification Number (VIN) | Registered Weight | Year | Make |
|  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| DIMENSIONS/WEIGHT | | | | | |  |
| Total | Length | Width | Height | Total Weight | Front Projection | Rear Projection |
| (max = 120’-0”) | (max = 16’-0”) | (max = 15’-5”) | (max = 80,000 lbs) | (max = 15’-0”) | (max = 15’-0”) |
|  |  |  |  |  |  |

**MAXIMUM AXLE WEIGHTS ALLOWED ON THIS PERMIT = 20,000 LBS PER AXLE**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| AXLE WEIGHTS/SPACINGS (REQUIRED FOR SME VEHICLES ONLY) | | | | | | | | | | | | | | | | |
| Axle Number | 1 (front) | | 2 | | 3 | | 4 | | 5 | | 6 | | 7 | | 8 | |
| Gross Axle |  | |  | |  | |  | |  | |  | |  | |  | |
| Weight (lbs) |
| Axle Spacing | |  | |  | |  | |  | |  | |  | |  | |  |

Applicant Signature: Approved By:

(Customer or Authorized Agent) Date Jones County Engineer’s Office Date

Maximum dimensions allowed and travel restrictions on an annual oversize permit are:

* 120’-0” long x 12’-5” wide x 13’-10” high – unlimited distance – no routing required
* 120’-0” long x 14’-6” wide x 15’-5” high – movement restricted to 50 miles radius unless the route continues on at least 4-lane roads or trip routes are obtained from Motor Carrier Services
* 120’-0” long x 16’-0” wide x 15’-5” high – trip routes must be obtained
* 75’-0” long x 12’-5” wide x 14’-6” high – maximum dimensions for hauling hay, straw, stover, and bagged livestock bedding

Carrier will be responsible for obtaining necessary route approval prior to move.

Permits can be issued only for transporting single articles that exceed statutory size limits unless the inclusion of additional articles does not cause the size or weight to further exceed the statutory limits.